Extruder:(moving arm) lang- space(2D) mai kaise move krna hai

Base – moves to make 2D->3D (if not and extruder moves in 3d space temp issues )

Material : PLA plastic

Leveling :quality assurance (origin or 0 defined )

Support material: which can be removed later on (dissolves in water) PVA polyvinyl (acetate)

Ted talk on 3D printer

Gcode – used for converting your design into printer readable format – design, printer specification

1. Cura
2. Slicer